Thanks for purchasing PLANET WGS-5225-8P2S Industrial L2+ 8-port 10/100/1000T 802.3at PoE + 2-port 1G/2.5G SFP Wall-mount Managed Switch.

This document provides the firmware release note and history of the product below:

Version 1.366b200722 was released on 07/22/2020
=======================================
Firmware version: v1.366b200722
Hardware version: 1.0
File Name: FW-WGS-5225-8P2S_v1.366b200722.dat
File Size: 6,725,632 bytes 
Released on 07/22/2020
=======================================

This firmware provides the following modifications:

A: Bug Fixed - N/A

B: Function added - 

1. Added port 9 and port 10 that support an operating speed of 2.5G.

[Note]
Hardware-based factory reset default is required for this firmware upgrade.
Press the hardware-based reset button on the device for about 10 seconds. 

[Upgrade Requirements]:

1. The latest firmware version of WGS-5225-8P2S.
2. The WGS-5225-8P2S switch.
3. Workstation with Microsoft IE 8.0 or above.

[Upgrade procedure]:

1. Connect the RJ45 UTP cable to the target switch.

2. Login is required to access the Web interface after the booting is completed successfully. The factory default user name and password are both "admin".

3. When the Web UI main screen appears, click System--> Web Firmware Upgrade" on the left side of the Menu.  

4. The screen provided HTTP firmware upgrading feature.

   A. HTTP Firmware Upgrade
     (1) Enter the "Browse.." button to locate firmware path.
     (2) Click the "Upload" button to start the firmware upgrade procedure. Please don't turn off the switch while procedure is processing.
     (3) Please wait for a while until the system reboot is completed.
     (4) Reset the switch to factory default and reboot it again.

   B.TFTP Firmware Upgared

     (1) Input TFTP server IP address to "TFTP Server IP" column and inputs firmware file name to "Firmware File Name" column. 
     (2) Click the "Upgrade" button to start the firmware upgrading procedure. Please don't turn off the switch while procedure is processing.
     (3) Please wait for a while until the "Complete" message shows on the web page.
     (4) Resets the switch to factory default and reboot system again.

5. Relog in the switch via Web browser. Please click the "System --> System Information" to check firmware version again if the firmware has been 
   upgraded successfully.


******************************
Firmware Release History:  
******************************

Version 1.366181023 was released on 10/23/2018
=======================================
Firmware version: v1.366181023
Hardware version: 1.0
File Name: FW-WGS-5225-8P2S_v1.366181023.dat
Released on 10/23/2018
=======================================

This firmware provides the following modifications:

A: Bug Fixed -
1: Fix compatible issue with SFP RJ45 copper module of other vendor.      
   
B. Function Added -
   NA

Version 1.366180130 was released on 01/30/2018
=======================================
Firmware version: v1.366180130
Hardware version: 1.0
File Name: FW-WGS-5225-8P2S_v1.366180130.dat
Released on 01/30/2018
=======================================

This firmware provides the following modifications:

A: Bug Fixed -
   NA    
   
B. Function Added -
1: Add manual time configuration function.
   
Version 1.366171121 was released on 11/21/2017
=======================================
Firmware version: v1.366171121
Hardware version: 1.0
File Name: FW-WGS-5225-8P2S_v1.366171121.dat
Released on 11/21/2017
=======================================

Initial Release
   
Sincerely yours,
PLANET Technical Support Team
Http://www.planet.com.tw







